Installing Supplemental Drivers on a Network
--------------------------------------------
This file is intended for system administrators or anyone
else who will install the drivers in this package onto a 
network for use with a shared copy of Windows.

1. Create a new directory on the network drive for the
   supplemental drivers you are going to install. It might be
   most convenient to make this directory a subdirectory of
   the Windows directory.

   This new directory should not be the Windows system directory,
   where the original Windows device drivers were installed.

2. Copy all of the files in the Supplemental Driver Library disks
   to the directory you created in step 1.

3. Copy all of the files in the new directory to the Windows
   directory.

   There will then be two copies of these files on your network
   drive. Both sets of drivers are necessary in order to ensure
   that these drivers will work properly on the users' systems.

4. Delete the file OEMSETUP.INF from the Windows directory.

   This ensures that this version of OEMSETUP.INF won't be 
   overwritten by another file with the same name.

   You should not delete the copy of OEMSETUP.INF that is in the
   directory you created in step 1.

Once these steps are completed, users of the shared copy of Windows
will automatically have access to these drivers.

The only exception is display drivers. To use one of the display
drivers included in this package, the user will need to run Setup
from MS-DOS using the following procedure. (This procedure is not
necessary for users who will not be using one of these display
drivers.)

1.  Exit Windows.

2.  Type the following at the DOS prompt and then press ENTER:

	setup /n 

3.  Press the UP ARROW key to select the Display setting and then
    press ENTER.

4.  Scroll to the bottom of the list using the DOWN ARROW key.

5.  Select Other and press ENTER.

6.  Type the pathname of the display driver and press ENTER.

    The driver will be located on the subdirectory created in
    step 1 of the previous set of instructions.
	
    Setup then updates your WIN.INI and SYSTEM.INI files to 
    correspond to the new driver and then displays an updated
    list of your hardware.

7.  Press ENTER to complete the process.

8.  Start Windows.  

The preceding procedure might not work if the user has a
local copy of Setup. In this case, the user will have to
manually change the settings in the SYSTEM.INI file and possibly
take additional actions. If you cannot use Setup /n to gain access
to a Supplemental Library display driver from the network, follow
the instructions that follow.

    
Manually Installing an SDL Display driver from a Network
to a Local Workstation
--------------------------------------------------------

You do not need to read the information in the following section
unless you were unable to use Setup to configure a user's system 
to use a Supplemental Library display driver that is on a 
network share.

  Printing this file:  You should print this file in landscape 
  mode (11 inches wide, 8.5 inches high) so that the table in
  this document will not run off the page.

To manually configure a workstation to gain access to an SDL display
driver on a network, follow these steps:

1.  Open your SYSTEM.INI file using a text editor, such as Notepad.
    This file should be located in your Windows directory.

2.  Locate the following four settings in SYSTEM.INI. In the [boot]
    section, locate the display.drv= and 386grabber= settings.
    In the [boot.description] section, locate the display.drv= setting.
    In the [386Enh] section, locate the display= setting.

3.  Look up the display driver you want to use in the following list and
    change the corresponding SYSTEM.INI values (the values are what
    appears to the right of the equal sign) to those shown on the list.
    
Name of display 				[boot]		[boot]		[386Enh]
(enter in [boot.description] display.drv=)	display.drv=	386grabber=	display=
-------------------------------------------------------------------------------------------
ATI Mode 54h (800x600 16 colors) v2.00		win3-54b.drv	vga.gr3		vddati.386
ATI Mode 55h (1024x768 16 colors v2.00		win3-55b.drv	vga.gr3		vddati.386
CHIPS Super VGA 82C451 (800x600 16 colors)	45131600.drv	vga.gr3		vddchip.386
CHIPS Super VGA 82C452 (800x600 16 colors)	45231600.drv	vga.gr3		vddchip.386
CHIPS Super VGA 82C451 (1024x768 16 colors)	win31768.drv	vga.gr3		vddchip.386
CHIPS Super VGA 82C452 (640x480 256 colors)	win3p480.drv	vgap45x.gr3	vddchip.386
COMPAQ Integrated Video Graphics System		cpqivgs.drv	vga.gr3		*vddvga
DGIS Medium Resolution w/VGA, Ver 1.01		dgis3lo.drv	dgisvga.gr3	*vddvga
DGIS High Resolution w/VGA, Ver 1.01		dgis3hi.drv	dgisvga.gr3	*vddvga
Paradise VGA (800x600 16 colors)		vga800.drv	vga.gr3		vddpara.386
Paradise VGA (1024x768 16 colors)		vga1024.drv	vga.gr3		vddpara.386
Paradise VGA (640x480 256 colors)		pvga480.drv	pvga.gr3	vddpara.386
Video Seven VGA (800x600 16 color)		v760016.drv	v7vga.gr3	*vddvga
Video Seven VGA (1024x768 16 color)		v776816.drv	v7vga.gr3	*vddvga
Video Seven VGA (640x480 256 color)		v7480256.drv	v7vga.gr3	*vddvga
-------------------------------------------------------------------------------------------

    Make sure you have correctly typed the appropriate values into your
    SYSTEM.INI file. 

4.  Save the new settings and close the SYSTEM.INI file.

5.  Exit Windows, if you have not already done so.

***************************************************************************
* IMPORTANT: If you are converting to one of the Supplemental Library     *
*      display drivers from a non-VGA driver, you will need to follow     *
*      steps 6 and 7.                                                     *
*                                                                         *
*      If your previous display was a VGA, you can skip to step 8.        * 
*  *********************************************************************  *
*                                                                         *
*  6.  Copy the files WIN.CNF, VGALOGO.LGO and VGALOGO.RLE from the       *
*      network Windows directory to your local Windows directory on       *
*      your hard disk.                                                    *
*                                                                         *
*  7.  At the DOS prompt, change to the local Windows directory and then  *
*      type the following commands:                                       *
*                                                                         *
*          copy win.cnf /b + vgalogo.lgo /b + vgalogo.rle /b              *
*                                                                         *
*  	   ren win.cnf win.com                                            *
*                                                                         *
***************************************************************************   

8.  Restart Windows.
